CDTV Memory Limits for Various CDTV

Configurations

Page XII - 17

Amiga Mail_{Volume II}

July/August 1992

Memory Limits for Various CDTV Configurations

by Adam Levin-Delson

RAM space is at a premium in the CDTV, so for the developer who is creating CDTV titles, it is important to know what the limits of system memory are. This is especially true for developers who want their titles to work on a variety of CDTV/A500 configurations. To help assist developers in making titles work on the maximum number of configurations, the following chart shows a variety of hardware configurations capable of playing CDTV discs.

For comparison purposes, all machines were allowed to boot far enough to open the Workbench screen (in the default size) and a CLI/Shell window. This represents a reasonable starting point for developers to estimate if their application will fit into a CDTV’s memory (To properly ascertain the amount of free memory in a particular CDTV/A500(+) at run time, use the Exec library’s AvailMem() function). These results are not guaranteed for any particular configuration, they can and will change depending upon many variables, including additional hardware, overscan or interlaced screens, etc. Use this information only as a guideline. Do not assume that these result will remain constant in future releases of the OS.

WARNING: A title that consumes too much memory on a current configuration may not work in the future if a new release of the OS consumes even a little more memory.

Important note about Workbench V1.3 and V 2.0. Under 1.3, the Workbench screen and initial CLI always open upon booting with an AmigaDOS disc. Under 2.0, the system only opens the Workbench screen when necessary, and only opens an initial CLI if the Startup-sequence attempts to output text. The C:Avail program first calculates the amount of free RAM and then prints out the results. Under 2.0, this means the amount of memory printed by Avail would differ from the amount of memory actually free by the amount needed to create the Workbench screen and initial CLI.

Machine NTSC/PAL 1.3/2.0 Peripherals * Available In-Use Maximum Largest

CDTV        NTSC      1.3    internal HD  c   799448     240704   1040152   797312
                             floppy
CDTV        NTSC      1.3    floppy       c   886688     153464   1040152   710472
CDTV        NTSC      2.0    floppy       c   840616     206936   1047552   689200
CDTV        NTSC      1.3    SCSI card    c   881248     158904   1040152   704904
CDTV        NTSC      1.3    floppy       c   878824     161328   1040152   878624
CDTV        PAL       2.0    floppy       c   807528     239992   1047520   792880
CDTV        PAL       2.0    none         c   828784     218768   1047552   824736
CDTV        PAL       1.3    floppy       c   877936     162216   1040152   710552
CDTV        PAL       1.3    internal HD  c   790488     249664   1040152   788352
                             floppy
A500/570    NTSC      1.3    internal FD  c   466256     56976    523232    466208
                                          f   412728     104160   516888    412552
                                          t   878984     161136   1040120   466208
A500/570    PAL       1.3    internal FD  c   457296     65936    523232    457248
                                          f   412704     104184   516888    412064
                                          t   870000     170120   1040120   457248
A500+/570   PAL       2.0    internal FD  c   809744     237776   1047520   795144
A500+       PAL       2.0    internal FD  c   839688     207864   1047552   838648
CDTV        NTSC      1.3    floppy       c   886688     153464   1040152   710472
CDTV        NTSC      2.0    floppy       c   840616     206936   1047552   689200
CDTV        NTSC      1.3    SCSI card    c   881248     158904   1040152   704904
CDTV        NTSC      1.3    floppy       c   878824     161328   1040152   878624
CDTV        PAL       2.0    floppy       c   807528     239992   1047520   792880
CDTV        PAL       2.0    none         c   828784     218768   1047552   824736
CDTV        PAL       1.3    floppy       c   877936     162216   1040152   710552
A500/570    NTSC      1.3    internal     c   466256     56976    523232    466208
                             floppy       f   412728     104160   516888    412552
                                          t   878984     161136   1040120   466208
A500/570    PAL       1.3    internal     c   457296     65936    523232    457248
                             floppy       f   412704     104184   516888    412064
                                          t   870000     170120   1040120   457248
A500+/570   PAL       2.0    internal     c   809744     237776   1047520   795144
                             floppy
A500+       PAL       2.0    internal     c   839688     207864   1047552   838648
                             floppy

* c=chip; f=fast; t=total
FD = Floppy Drive; HD = Hard Drive

∞∞ CDTV Memory Limits for Various CDTV Configurations

Page XII - 18

Amiga Mail_{Volume II}