PROCESSOR Intel 486DX4/100 upgradeable to Intel Pentium OverDrive Microprocessor

UPGRADABILITY Allows upgrade of processor and memory

GRAPHICS Canon Proprietary Video Architecture 2-MB VRAM standard -1280x1024 with 16-bit color and 72 Hz max vertical refresh rate -1152x900 with 4,000 colors with 16-bit color and 82 Hz max vertical refresh rate -1120x832 with 16-bit color and 90 Hz max vertical refresh rate -1024x768 with 16-bit color and 98Hz max vertical refresh rate- -800x600 with 32-bit color and 110Hz max vertical refresh rate -640x480 with 32-bit color and 110Hz max vertical refresh rate

INTEGRATED AUDIO Integrated CD-quality audio (16- bit, 44Khz stereo), speaker, microphone and software that allows voice annotation, voice recognition, and audible proo�ng. Sound blaster capability

INTEGRATED LOCAL NETWORK INTERFACE CONTROLLER 32-bit Ethernet controller located on VL bus. Bus Mastering capabilities, jumperless and switchless setup, and RJ-45 connector.

INTEGRATED VL FAST SCSI-2 CONTROLLER 32-bit Fast SCSI-2 controller located on VL bus. Up to 10 MB per second data transfer rate.

ADVANCED ERGONOMIC DESIGN High video refresh rate Slim-line chassis with side-entry removeable media Noise Reduction System

MEMORY 16MB RAM expandable to 96MB via industry standard 72-pin SIMM modules

ARCHITECTURE VL Bus and Industry Standard Architecture (ISA)

INTERNAL EXPANSION SLOTS Three ISA expansion slots One VL/ISA (typically used for SCSI controller)

INTERFACES Fast-SCSI-2; RJ-45 (for Ethernet); parallel; two serial; standard keyboard and pointing device (mouse) connectors. External jacks for video, headphone, microphones, stereo speakers, and auxiliary multimedia devices.

TOTAL STORAGE CAPACITY One 5.25-inch half-height user accessible drive bay. One 3.5-inch third-height user accessible drive bay dedicated to floppy Two 3.5-inch third-height or one 3.5-inch half-height internal drive bay DISKETTE DRIVE One 3-1/2-inch 1.44-MB diskette drive standard on all models

CACHE 16-Kbyte internal cache, writethrough cache. 256-Kbyte external cache, writethrough cache.

ENERGY SAVING FEATURES Intelligent energy saver mode for monitor

KEYBOARD Canon keyboard with NeXTspeci�c keycaps, controls for audio volume and monitor brightness

POINTING DEVICE Canon PS/2-style mouse standard

ACOUSTICS AND THERMAL MANAGEMENT Incorporates new multi-fan system to enable a quieter system operation while maximizing component cooling

SECURITY Power-on password

S T A N D A R D F E A T U R E S

For more information about the Canon object.station 41, give us a call at [800] 349-6007. Or for instant faxed hard copy, call our Canon FactsLine at [800] 526-4345.

POWER SUPPLY AC voltage: 95-130VAC, or 180- 270 VAC Frequency: 50Hz to 60Hz 180 watts steady state output

PREINSTALLED SOFTWARE NEXTSTEPfor Intel Processors, user license (includes CD-ROM and documentation) Insignia�s SoftPC Demo Version

SERVICEABILITY Easy access system design via thumb screws No special tools required

SERVICE AND SUPPORT Canon provides a wide range of service offerings including a 1- year limited warranty with on-site service; toll-free 7 x 24 technical phone support; access to Canon FactsLine for faxed document retrieval

O P T I O N S

PROCESSOR Pentium Upgrade Kit

MEMORY 16-MB Memory Kit

PREINSTALLED SOFTWARE NEXTSTEP Developer (includes CD-ROM and documentation) Microsoft DOS Microsoft Windows

STORAGE DEVICES 500-MB Fast-SCSI-2 Internal Hard Drive 1-GB Fast-SCSI-2 Internal Hard Drive Double-Spin Internal CD-ROM Drive

MONITORS 17-inch Color Monitor, .26mm dot pitch, Low Emissions (MPR II compliant) 21-inch Color Monitor, .28mm dot pitch, Low Emissions (MPR II compliant)

'1994 Canon Computer Systems, Inc. Canon is a registered trademark of Canon Inc. All other products are registered trademarks of their respective companies. Specifications are subject to change without notice. Printed in the U.S.A.

obj ect.sta tion 41