Supported System Software: 7.5.2
SCSI: HDI-30
Serial Ports: 1
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: AAUI-15
Machine Gestalt ID: 126

Minutiae:

NO LONGER AVAILABLE.  The 117 MHz NUpowr PowerPC upgrade has been replaced by a 167MHz version.

The NUpowr card uses approximately the same amount of power as the 68040 card it replaces.

The three versions of NUpowr differ only in the amount of soldered on RAM.  The 0K version is for users who have 16MB or larger memory modules.  The 4MB version is for users with 8MB or larger memory modules.  The 8MB version is for users with 4MB or larger memory modules.

NUpowr works with existing PowerBook 500 memory modules if the memory modules were designed correctly.

Original Enabler: PowerBook 5300/2300/190 enabler

Has 4 MB ROM