SCSI: DB-25
Serial Ports: 2
Sound Output: 16-bit stereo 44.1 KHz sample rate
ADB: 1, plus additional port for PS/2 keyboard
Ethernet:  Add-in card
Machine Gestalt ID: ??

Minutiae:

Accelerate performance with a Newer Technology 512KB Cache DIMM, part # 7CC512C.

PowerBase can take only 5 volt EDO DIMMs, not 3.3 volt.  It does not support interleaved memory.  The three DIMM sockets are NOT identical.  The first socket can only accept up to 32 MB DIMMs.  The other two sockets can accept up to 64 MB DIMMs.  The maximum memory is therefore 160 MB.

Manufactured by:
Power Computing Corporation
1-800-769-5917
info@powercc.com
http://www.powercc.com