SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: optional
Machine Gestalt ID: ??

Minutiae:

Due to conflicting information from UMAX, Newer Technology is recommending the use of EDO memory.  UMAX’s website says either FPM or EDO will work.  Their manual says only EDO will work.  The machine that the text you are reading is being composed on is a C600 with a 64 MB FPG DIMM installed.

Memory system is non-interleaved.

Manufactured by UMAX Computer Corporation
Toll-free tech support at 1-888-600-4400
Online system support at www.supermac.com