InS_StArT
DEFEA.COM
1.0
^DEC FDDIcontroller/EISA (DEFEA),DEFEA.COM,0E0,DEC3002
?The DEC FDDIcontroller/EISA DOS ODI Client Driver is the terminate-stay-resident (TSR) device driver for the DOS environment.  This driver works with the DEC FDDIcontroller/EISA Fiber or UTP adapter.
$O0E0(SLOT)Slot Number
1
15
$O0E0(MAX FRAME SIZE)Max Frame Size ( default = 4491 )      
?Enter the maximum frame size for this adapter.  Normally the driver advertises the maximum frame size allowed for FDDI (4491 bytes) but this parameter may be used to lower the setting.
16
4491
@4491
$O0E0(TREQ)Requested TTRT  ( default = 8 )                      
?Enter the desired MACTReq value in milliseconds.  Normally this parameter does not need to be changed from the default value of 8 ms.
4
165
@8
!O0E0(FULLDUPLEX)Full-Duplex Mode (default=OFF)   
?Enter whether FDDI Full-Duplex (FDX) mode should be enabled on the adapter.
@OFF
ON
$O0E0(NODE ADDRESS)Node Address
0
FFFFFFFFFFFF
*R0E0(FRAME)Media Frame Type(s)                                 
@FDDI_802.2
FDDI_SNAP
InS_EnD
