InS_StArT
DEFPA.COM
1.0
^DEC FDDIcontroller/PCI (DEFPA),DEFPA.COM,000
?The DEC FDDIcontroller/PCI DOS ODI Client Driver is the terminate-stay-resident (TSR) device driver for the DOS environment.  This driver works with the DEC FDDIcontroller/PCI Fiber or UTP adapter.
$O000(PCICARD)PCI Card Number ( default = 1 )                   
?Enter the PCI card (instance) number of the DEC FDDIcontroller/PCI adapter for this bus number.
1
4
@1
$O000(PCIBUS)PCI Bus Number  ( default = 0 )                    
?Enter the PCI bus number where the desired DEC FDDIcontroller/PCI adapter is installed.  For single-PCI bus systems, this value is zero (0).
0
255
@0
$O000(MAX FRAME SIZE)Max Frame Size ( default = 4491 )      
?Enter the maximum frame size for this adapter.  Normally the driver advertises the maximum frame size allowed for FDDI (4491 bytes) but this parameter may be used to lower the setting.
16
4491
@4491
$O000(TREQ)Requested TTRT  ( default = 8 )                      
?Enter the desired MACTReq value in milliseconds.  Normally this parameter does not need to be changed from the default value of 8 ms.
4
165
@8
!O000(FULLDUPLEX)Full-Duplex Mode ( default = OFF )   
?Enter whether FDDI Full-Duplex (FDX) mode should be enabled on the adapter.
@OFF
ON
*R000(FRAME)Media Frame Type(s)                                 
@FDDI_802.2
FDDI_SNAP
InS_EnD
