MBM 5.3.4.0

	MBM 5 Core EXE		 : 5.3.4.0
	MBM 5 Core DLL 		 : 5.3.4.0
	MBM 5 Settings DLL		 : 5.3.4.0
	MBM 5 Dashboard DLL		 : 5.3.4.0
	MBM 5 Hibernation DLL		 : 5.0.0.0
	MBM 5 Ras DLL		 : 5.0.0.0
	MBM 5 Logger DLL 		 : 5.3.4.0
	MBM 5 Mail, FTP and UDP DLL	 : 5.3.4.0
	MBM 5 OSD DLL		 : 5.0.0.3
	MBM 5 ASPI DLL		 : 5.2.1.0
	MBM 5 Heat Up EXE 		 : 5.0.0.0
	MBMIO DLL			 : 1.0.0.2

Changes from MBM 5.3.4.0

  added:
	- Winbond W83647HF (thank you Winbond)
	- Increased support for the EPIA boards (VT1211)
	  thank you VIA Germany and ACME.de
	- Configuration wizard, the reason for the increase 
	  in size of the d/l.
	- Special dump on the system info tab used to
	  add your board to the config wizard for other
	  users.	
	- wm_pause and wm_resume message (see
	  help file advanced - messages)
	- Priority function added to the starter.dll
	- SetPath function added to the starter.dll in case
	  you plan on running it as a service and it has no
	  access to HKEY_CURRENT_USER in the reg.
	- 2nd CPU temp on GA-7DPXDW+ which uses 
              1 LM90 for 2 CPU's (big thanks to Tim South for
	  keeping at it)
	- templist.ini added, with this you can enter your
  	  own temp table, see the help file advanced section
    
  Fixes:
	- installer would always recommend C:\program files
 	  even if your program files was on another drive, this
	  should be fixed now
	- autohide dashboard did not always work 100% when
	  you had the dashboard set to start with MBM
	- problem with e-mail test button
	- dual monitor and OSD, the slided will now allow you
	  to select a position on the left monitor
	- problem with ADM1030 fan speed (Charles Xuereb)
	- the LPC47xxx group of fans should respond better 	
	  to the do not reset sensor chip option
	- ITE range of sensors fan sensor 3 dividor problem 
	  fixed (thanks Anthony Smith)
    
  Changes:
	- installer offers to start MBM after install
	- installer will offer (checked) to start the help file
	  if it's a new install
	- installer will offer (unchecked) to start the help file
	  if it's an update install
	- ICH4-M auto enabled
	- English language file (thanks Wesley Chung)
	- fantemplist.ini has been changed, you now need
	  to make a file for each fan you want to base a 
	  a temp sensor on, so fantemplist1.ini if you want
	  to use fan1, fantemplist2.ini if you want to use
	  fan 2
	- fantemplist increased to 16
   
  voltage.ini
	- GA-8IPE1000Pro 
         	- SOYO DRAGON KT400 (VTech) 
	- GA-8KNXP (MeanGene)
	- EPoX 8RDA/8RDA (Valery Shatunov)
	- Elite L7S7A2 (Willem Schaaij)
	- Biostar M7VIG PRO (Chris Christo)
	- Asus A7V8X-X (Willem Schaaij)