;
; Advanced Call Center (ACC), (c) 1998 - 2000 Oleg Afonin
;

[Options]

;
; Better setup
;
nTAPI=1

; Default modem name
;   Type: string
;   Default: 'Default modem'
;   Comment: Change this value, run and exit program - new section
;            will be created. Change all parameters there
;
; If you want to edit modem profile, select 'Custom' and edit [Custom] section
;
sModem=LT Win Modem

; COM port number.
; Modem serial (COM) port
;  Range: -1, 1, 2, 3 or 4
;  Default: -1 (auto)
;
nComPort=-1

; Line source.
;  Range:
;   0		remote (default)
;   1		handset
;   2		mic
;   3		speaker
;   4		monitor
;   5 (or 6)	speakerphone
;  Default: 0
;
nLineSelection=0

; CID type
;  Range: 0 - 3
;  0 - Russian CID (default)
;  1 - Hardware (modem-specific) CID (supported in special cases only)
;  2 - USA CID standard
;  3 - other (reserved)
;
nCIDType=2

; Get CID in real-time. This causes CID be detected FASTER and, in some cases, better.
;  Range: boolean (1 or 0)
;  Default: 0
;
bRealTimeCID=1

; Time to wait for CID beginning when real-time CID is enabled
; Increase if a lot of numbers can't be detected
;  Range: 200 - ~2000 
;  Default: 340
;
dwTimeToWait=340

; Voice (CID) record time (milliseconds) 
; Increase if a lot of numbers can't be detected
;   Range: 500 - 10000 
;   Default: 3000 (try 1500 if frequent detection errors occure)
;
dwTimeToGet=4500

; While in 'delay before CID request' state, detect CID presense
;  Range: boolean (1 or 0)
;  Default: 1
;
bActiveDelay=0

; Voice (CID) record time (milliseconds) IMMEDIATELY after answer.
; Useful on SOME ATS' which send CID _before_ they receive CID request.
; Decrease or ZERO if a lot of numbers can't be detected
;  Range: 500 - ~2000 
;  Default: 100 (in some cases 750-1000 is good enough)
;
nPreDetectTime=15

; Online inactivity timer (milliseconds).
;  Range: 0 - MAXDWORD
;  Default: 60000 (1 minute of inactivity causes line drop)
;
dwInactiveTimer=60000

; When using new method of playing message through the line,
; specifies time of one block played.
;  Range: ~10 - ~60000 (milliseconds)
;  Default: 20 ms
;
nBlockTime=40

; Number of CID requests (tone beeps) sent per ONE detection cycle.
;  Range: 1-2
;  Default: 1 (try 2 if does not work)
;
nCIDReqNumber=1

; Use short (100 ms instead of 200 ms) CID request
;  Range: boolean (0 or 1)
;  Default: 0
;
bShortRequest=0

; Maximum number of attempts to get CID if previous attempt failed.
; Can cause an extra time before replying when CID can't be detected.
;  Range: 1-3 (3 is the maximum that ATS allows)
;  Default: 2
;
nMaxAttempts=2

; Clear Comm Error after each read/erite operation
;  Range: boolean (0 or 1)
;  Default: 0
;
bSafeIO=0

; Overlapped I/O.
;  Range: boolean (0 or 1)
;  Default: 0
;
bOverlappedIO=1

; Default timeout for all operations. It is the UPPER time limit (milliseconds)
; the program will wait for modem' response on command.
;  Range: 0 - 3000
;  Default: 2500 (try 820 with Quant=15)
;
dwTimeoutDefault=2500

; Default timeout for single character operations (milliseconds)
; Set together with 'default timeout (dwTimeoutDefault)'.
; Program uses this value to determine its time slice in a single-character operations
;  Range: 0 - 2000
;  Default: 15 (try 5 with Default=145)
;
dwTimeoutQuant=55

; Use hardware to detect ring. Turn this off for compatibility
; reason if the program does not detect ring.
;  Range: boolean (0 or 1)
;  Default: 1
;
bUseHardwareRing=0

; Action after handset pickup.
;
nAction=0
nWhiteAction=1000
nBlackAction=2

; Try faster initialization algorythm. Generally recommended.
; Should be disabled during debugging proceess.
;
bFasterModemInit=1

; Fourier window shift stepping (samples)
; Used in caller number detection algorythm. Less is more time consuming,
; but may be more accurate (set 'nDetectFakeDigits=-1' if you change this).
;  Range: -1 - ??
;  Default: -1
;
step=-1

; Serial baud rate (bits per second)
; Do not change this one!
;  Range: 2400 - 115200
;  Default: 19200
;
dwBaudRate=256000

; Number of rings before trying to detect CID
; 0 - do not answer automatically
;  Range: 0 - 6
;  Default: 1
;
nRings=2

; Number of wait signals sent to line before hangup
;  Range: 1 - ?
;  Default: 6
;
nWaitSignals=0

; Debug level. Stores intermediate information in files.
; - mode 0: no debug info saved
; - mode 1: PCM data saved in the prog's folder with temporary generated
;           filenames, including 'Real-time CID'.
;           Detected numbers saved there too. 
;           All files are being deleted after program exit except
;           'modem.log' file created.
; - mode 2: PCM and Compressed Voice data saved.
;           PCM is not saved with 'Real-time CID' enabled.
;           Detected numbers saved. Detected ATS
;           packet digits saved. Deleted after exit.
;           'modem.log' created.
;  Range: 0, 1 or 2
;  Default: 0
;
nDebugLevel=0

; Separate digits - smart method. Use by default.
;  Range: boolean (0 or 1)
;  Default: 1
;
bSmartDigitExtraction=1

; Threshold value to separate digits.
;  Range: 0 (don't use) to ~255
;  Default: 26
;
nSmartDigitExtractionThreshold=26

; False (errorneous) digits detect. Increase this if detected number
; contains _more_ digits than the real one; decrease if less digits in
; detected number than in real one
; -1 means automatic garbage collection (if this does not work correctly,
; try to set this explicitly to 2 or 3)
;  Range: -1 (auto), 0 - ~10
;  Default: 2
;
nDetectFakeDigits=-1

; Number of digits in the phone numbering system at your location.
;  Range: usually something between 5 and 7
;  Default: 7
;
nDigitsInNumber=7

; Start disabled (paused).
;  Range: boolean (0 or 1)
;  Default: 0
;
bStartDisabled=0

; Detect cadence (busy signal) while being online (talking) or sending
; 'wait' signals to remote caller. If cadence detected, hangs up the modem.
;  Range: boolean (0 or 1)
;  Default: 1
;
bCadenceDetection=1

; Period of cadence detection.
; Less values maybe less precise but give faster response.
;  Range: 100 - 4000
;  Default: 2000
;
dwCadenceQuant=4000

; Check incoming ring event whether it was a real ring ("RING" modem response) or not.
; May cause some rings not to be handled. Prevents most of pulse dialing on a parallel
; phone device from being treated as incoming rings.
;  Range: boolean (0 or 1)
;  Default: 1
;
bConfirmRing=1

; Show notification dialog (info on Caller and Phone number) when detected CID.
;  Range: boolean (0 or 1)
;  Default: 1
;
bShowNotificationDlg=1

; Use alternative way of delivering commands to modem.
; May be faster and more compatible with your modem.
; Try 0 if commands are NOT accepted by your modem.
;  Range: boolean (0 or 1)
;  Default: 1
;
bUseAltCmdTransmit=1

; Save log file
;  Range: boolean (0 or 1)
;  Default: 1
;
bSaveLogFile=1

; Name of the log file. Use relative or full path and file name.
;
sLogFileName=logfile.txt

; Use external files to utilize help.
; Greatly reduces memory usage.
;  Range: boolean (0 or 1)
;  Default: 0
;
bUseExternalHelp=1

; Show dialog tips
;  Range: boolean (0 or 1)
;  Default: 0
;
bShowDlgTips=0

; Ring emulation frequensy.
;  Range: 300-3000
;  Default: 425
;
nFreqRing=480
nFreqRing2=620

; Length of RING emulation tone in Russian CID
;  Range: integer (Standard1: 800 Standard2: 1000)
;  Default: 800
;
nRingEmulationLength=800

; Pauses between RING emulation tones in Russian CID
;  Range: integer (Standard1: 3000 Standard2: 4000)
;  Default: 3000
;
nRingEmulationPause=3000

; Turn on modem speaker while answering
;  Range: boolean (0 or 1)
;  Default: 0
;
bEnableModemSpeaker=0
	
; Use software (sinusoidal) tone generator (more precise timing)
;  Range: boolean (0 or 1)
;  Default: 0
;
bSoftwareToneGenerator=0

; Exact CID request time.
;  Range: integer (40 - 300), recommended (90 - 160)
;  Default: 160
;
nReqTime=160

; Pop-up window font size(14 or 15)
;
g_iFontHeight=15

; Monitor voice from modem to sound card
;  Range: boolean (0 or 1)
;  Default: 0
;
bEnableSBOutput=0

; Monitor the messages played to the line via sound card
;  Range: boolean (0 or 1)
;  Default: 0
;
bEnableSBOutput_play=0

; Format phone number for better display (i.e. "1234567890" to "(123) 456-7890")
;  Range: boolean (0 or 1)
;  Default: 1
;
bReFormatNumber=1

; LCD background index
;
LCD_bk=1

; Monitor DTMF tones
;  Range: boolean (0 or 1)
;  Default: 1
;
bEnableDTMFDetection=1

; Use fast line signals detection.
;  Range: boolean (0 or 1)
;  Default: 0
;
bUseFastDTMFDetection=1

; Hardware AGC (Automatic Gain Control)
;  Range: boolean (0 or 1)
;  Default: 0
;
iAGC=0

; Software AGC (Automatic Gain Control)
;  Range: boolean (0 or 1)
;  Default: 1
;
bSoftAGC=0

; Russian CID request frequency
;  Default: 500 Hz
;
iReqFreq=500

; How much times per second to interrupt PLAYBACK
; to scan line signals.
;  Default: 10 Hz
;
iScanFreq=1000

; Max block size that will be written to modem continuously.
;  Default: 4096 bytes
;
iMaxBlockWrites=16384

; Generated tone volume
;  Range: 0 - 100
;  Default: 100
;
iToneVolume=100

; Use compatible sound playback. Set this when getting
; chopping sound while playing through modem line in pass-through mode.
;  Range: boolean (0 or 1)
;  Default: 0
;
bCompatiblePlayback=1

; Use fixed font. Compatibility option. Change state if troubles with font displaying.
;  Range: boolean (0 or 1)
;  Default: 1
;
g_bFixedFont=1

; Single click toggles pause.
;  Range: boolean (0 or 1)
;  Default: 1
;
bClick=0

; Defaults for telephone number formatting
sFormat5=%c%c%c%c%c
sFormat6=%c%c%c-%c%c%c
sFormat7=%c%c%c-%c%c%c%c
sFormat8=%c%c%c%c-%c%c%c%c
sFormat9=%c%c%c%c%c-%c%c%c%c
sFormat10=(%c%c%c) %c%c%c-%c%c%c%c
sFormat11=%c (%c%c%c) %c%c%c-%c%c%c%c
sFormat12=(%c%c%c%c%c) %c%c%c %c%c%c%c
sFormat13=%c%c%c %c %c%c%c%c %c%c%c%c%c

; Available format strings
;         1-23-45;     12345;     12-345;     1 2345
saFormat5=%c-%c%c-%c%c;%c%c%c%c%c;%c%c-%c%c%c;%c %c%c%c%c
;         12-34-56;      123 456;      12 3456
saFormat6=%c%c-%c%c-%c%c;%c%c%c-%c%c%c;%c%c %c%c%c%c
;         123-45-67;       123-4567 Israel
saFormat7=%c%c%c-%c%c-%c%c;%c%c%c-%c%c%c%c
;         1324 5678        ;(12) 345678;        (1) 234-5678
saFormat8=%c%c%c%c-%c%c%c%c;(%c%c) %c%c%c%c%c%c;(%c) %c%c%c-%c%c%c%c
;         12345 6789;         1234 56789;         ++12-3-456789 (Italy); (12) 345-6789 (Israel);(123) 456-789 Israel mobile
saFormat9=%c%c%c%c%c %c%c%c%c;%c%c%c%c %c%c%c%c%c;++%c%c-%c-%c%c%c%c%c%c;(%c%c) %c%c%c-%c%c%c%c;(%c%c%c) %c%c%c-%c%c%c
;          (123) 456-7890 (US,CA,JP);+1 (23) 456-78-90 (RU);    (+12)-3456-7890 (Germany);+12 34 56 78 90 France, Nd;1234 567 890 AU mobile;1234 567890 GB mobile;(+12) (3) 456 78 90 Belguim;(+12) 3456 7890 (Dutch);   +12 3 456-7890 (Spain);  +12 34 567890 (Spain);  +12-3-4567890 (Sweden); 123-456-7890;            12 3456 7890 Australian
saFormat10=(%c%c%c) %c%c%c-%c%c%c%c;+%c (%c%c) %c%c%c-%c%c-%c%c;(+%c%c)-%c%c%c%c-%c%c%c%c;+%c%c %c%c %c%c %c%c %c%c;(%c%c%c%c) %c%c%c %c%c%c;%c%c%c%c %c%c%c%c%c%c;(+%c%c) (%c) %c%c%c %c%c %c%c;(+%c%c) %c%c%c%c %c%c%c%c;+%c%c %c %c%c%c %c%c%c%c;+%c%c %c%c %c%c%c%c%c%c;+%c%c-%c-%c%c%c%c%c%c%c;%c%c%c-%c%c%c-%c%c%c%c;%c%c %c%c%c%c %c%c%c%c
;          +1 (234) 567-89-01 (RU);      (12) (3) 45 67 89 01 (France);  +12-3-45-67-89-01 (France); +12 3 4567 8901 (AU);       (+12) 3 4567 8901 (AU);      1234 567 8901 (GB, London);12345 678901 (GB,other);(1)2345 67 89 01 (GB,IR?);(12345) 678901 (GB,IR?); +12 34 567 8901 Netherlands;(+12) 34-567 89 01 Netherlands;(123) 4567-8901 Hong Kong;+123-4-5678901 (Finland);+12.3.4567.8901 (Japan);    USA, Canada 1 (234) 567 8901;(12345) 678901;          (1234) 567-8901
saFormat11=+%c (%c%c%c) %c%c%c-%c%c-%c%c;(%c%c) (%c) %c%c %c%c %c%c %c%c;+%c%c-%c-%c%c-%c%c-%c%c-%c%c;+%c%c %c %c%c%c%c %c%c%c%c;(+%c%c) %c %c%c%c%c %c%c%c%c;%c%c%c%c %c%c%c %c%c%c%c;%c%c%c%c%c %c%c%c%c%c%c;(%c)%c%c%c%c %c%c %c%c %c%c;(%c%c%c%c%c) %c%c%c%c%c%c;+%c%c %c%c %c%c%c %c%c%c%c;(+%c%c) %c%c-%c%c%c %c%c %c%c;(%c%c%c) %c%c%c%c-%c%c%c%c;+%c%c%c-%c-%c%c%c%c%c%c%c;+%c%c.%c.%c%c%c%c.%c%c%c%c;%c (%c%c%c) %c%c%c %c%c%c%c;(%c%c%c%c%c) %c%c%c%c%c%c;(%c%c%c%c) %c%c%c-%c%c%c%c
;          +12 (3)45 678 90 12 (AU, Netherl); +12 3 45/67 89-012 (Germany);+12 345/67 89-012 (Germany);  +12-(3)-4567-8901-2 (Germany);  +12 (3) 45 678 9012 (Germany);  (+12)(3) 4567 8901 2 (Germany);+12 (3)456 789012 (Germany);  (+12) 34 56 78 90 12 (France);   +12 (3)45 678 90 12 (AU?);      12 345 6789012 (GB?);      +12 3456 789012 (GB?);      +12 (3)45 6789012 Netherlands
saFormat12=+%c%c (%c) %c%c %c%c%c %c%c %c%c;+%c%c %c %c%c/%c%c %c%c-%c%c%c;+%c%c %c%c%c/%c%c %c%c-%c%c%c;+%c%c-(%c)-%c%c%c%c-%c%c%c%c-%c;+%c%c (%c) %c%c %c%c%c %c%c%c%c;(+%c%c)(%c) %c%c%c%c %c%c%c %c;+%c%c (%c)%c%c%c %c%c%c%c%c%c;(+%c%c) %c%c %c%c %c%c %c%c %c%c;+%c%c (%c)%c%c %c%c%c %c%c %c%c;%c%c %c%c%c %c%c%c%c%c%c%c;+%c%c %c%c%c%c %c%c%c%c%c%c;+%c%c (%c)%c%c %c%c%c%c%c%c%c
;          (123) 456-7890123 (def);       (+12)(3) 4567 8901-23 (Germany);   +12 (3)4567 89 01 23 (GB, Ireland?)
saFormat13=(%c%c%c) %c%c%c-%c%c%c%c%c%c%c;(+%c%c)(%c) %c%c%c%c %c%c%c%c-%c%c;+%c%c (%c)%c%c%c%c %c%c %c%c %c%c

; Use text-to-speech engine.
;  0 - do not use
;  1 - use Voice TTS API
;  2 - use instant Voice TTS API
;  3 - use on-load Voice TTS API (does not work)
;  1001 - use Direct TTS API
;  1002 - use instant Direct TTS API
;  1003 - use on-load Direct TTS API (does not work)
;
nTextToSpeech=0

; Software 'busy' detection..
;  Range: boolean (0 or 1)
;  Default: 1
;
bSoftBusy=0

; Part of all blocks to analyze for 'busy' tone.
;  Range: 1 - 10
;  Default: 2 (1/2 of all blocks to analyze)
;
iBusyDiscrete=2

; Detect 'busy' after there were several tones.
;  Range: 1 - 10
;  Default: 2
;
iBusySignal=2

; Time of one 'busy' tone (ms)
;  Range: usually 150 - 300
;  Default: 150
;
iBusyTime=150

; Caller ID with phone number only (no caller name transmitted).
;  Range: boolean (0 or 1)
;  Default: 0
;
bNumberOnlyCID=0

; Perform extra port initialization: queue setup.
;  Range: boolean (0 or 1)
;  Default: 0
;
bSetupQueue=0

; Size of internal communication buffer. */
;
QUEUE_SIZE=1024

; Journal originated calls.
;  Range: boolean (0 or 1)
;  Default: 1
;
bLogOriginatedCalls=1

; Ring (play sound through a sound card) with a standard RING
; before the caller is detected and customized RING sound can be played back.
;  Range: boolean (0 or 1)
;  Default: 0
;
bRingBeforeCallerID=1

; Turn on silence detection.
;  Range: boolean (0 or 1)
;  Default: 1
;
bSilenceDetection=1
iSilenceDetectionSensitivity=50
iSilenceDetectionTimeout=5

; Area codes map. Empty sets the appropriate map automatically.
; The map must be stored in <acid2000>\areacode folder.
;
sAreaMapDB=US.db
; Announce state and major cities for long-distance calls.
bAnnounceState=1
bAnnounceCities=0

; Heuristic in phone number formatting (mobile phones detection and so on).
;  Range: boolean (0 or 1)
;  Default: 1
;
bAdvancedFormatting=0

; Pop-up dialog new design style.
;  Range: boolean (0 or 1)
;  Default: 1
;
bNewDesign=1

; Use dialing rules
;  Range: boolean (0 or 1)
;  Default: 0
;
bUseAreaRules=0

arRASWindows=Dial-Up Networking;Dial-up Connection;Connect To;Dialing Progress;Connecting to;Connessione a

; Track handset pick-up
;  Range: boolean (0 or 1)
;  Default: 0
;
bTrackHandset=0

; VRA, 1/10 of second
nVoiceRingbackGoesAway=70
; VRN, 1/10 of second
nVoiceRingbackNeverCame=100
ld_prefix=
AlwaysDialAll10=0
bPulseDial=0
bTreatZeroNumberAsUnknown=0
bDropBlackCalls=0
bFax=0
sFaxAppName=
sFaxParam=
uiFaxSeconds=30
bDisableModemInact=1
bCompat=0
iPopup=0
dwPopupTimer=15000
bStoreWavLogs=1
AlwaysDial1=
DontDial1=
nFigures=7
bCompatibleDial=0
AreaCode=
bKeepSpeaker=1
bRecordOriginated=0
bEMailCID=0
bEAttachVoice=0
bEDialUp=0
bECIDSubj=0
nEWaitSeconds=30
m_sOriginatorName=
m_sOriginatorAddress=
m_sRecipsName=
m_sRecipsAdderss=
m_sSubject=
m_PagerType=0
m_PagerPort=1
m_PagerRetries=1
m_PagerDelay=10
m_PagerBlock=80
m_PagerAccount=
m_PagerMessage=
m_PagerPhone=
m_PagerSerialSetting=1200,E,7,1
TTS_bEnable=0
TTS_bIncoming=1
TTS_bName=1
TTS_bNumber=1
TTS_bOnlyName=0
TTS_bSpellNA=1
TTS_times=1
TTS_sIncoming=Incoming call:
TTS_sName=Caller is
TTS_sNumber=Telephone number is
TTS_index=0
DTMF_0=0
DTMF_1=0
DTMF_2=0
DTMF_3=0
DTMF_4=0
DTMF_5=0
DTMF_6=0
DTMF_7=0
DTMF_8=0
DTMF_9=0
DTMF_A=0
DTMF_B=0
DTMF_C=0
DTMF_D=0
DTMF_STAR=0
DTMF_NUM=0
bFlashKeyb=0
bPinDial=1
nTAPILine=7
bShowCidName=0
bSwapName=0
bUnattendedPage=1
m_nPIN=0
bPinTTS=0
bPinInstruct=1
bPinRequest=1
bPinConfirm=1
sPinInstruct=
sPinRequest=./wave/Passwrdq.wav
sPinConfirm=
bScheduleGreeting=0
sScheduleGreeting=
bAlphaConvert=1
bRecAll=1
bHandsetStart=0
bHandsetStop=0
bHilightNew=1
bPageContactsOnly=0
bUseSoundIntervals=0
iSoundInterval=60
sWaveNewMessage=
bEMailCompress=0
bTollSaver=0
strPinArray=
sWaveRemoteGlobal=wave\silence.wav
sWaveSilence=wave\silence.wav
sWaveNoNewMessages=wave\nonewmsg.wav
bIgnoreBusy=0
bRunProg=0
bRunAfter=0
bRunDisableBlack=1
bRunPause=0
sRunApp=
sRunParam=call.number" "call.name
bRunNotAnsw=0
nFwdMethod=0
bFwdBlack=0
sFwdPhone=
dwDialFor=60000
m_iVolume=50
strVersion=4. 0. 0. 592
nFreqRing3=500
nFreqRing4=67
bUseWindowSchedule=1
bFlashOnNewMsg=0


[Sounds]
; Wave: incoming ring sound
sWaveRingIn=Wave\Ringin.wav
	
; Wave: sending 'wait' signals
sWaveWait=wave\ringout.wav
sWaveHold=wave\hold.wav
sWaveCompressedHold=wave\hold.wav
; Wave: 'default greeting'
sWaveGreet=wave\greet.wav
; Wave: 'alternative greeting'
sWaveAltGreet=wave\block.wav
sWaveGreet2=wave\greet.wav
sWaveClick=wave\signon.wav

; Program startup options
[Startup]
dwVersion=40000

; Show 'Main' dialog during startup
ShowMainDlg=1
; Screen coordinates of CallerID pop-up window.
; Default: (-1, -1)
iPopupX=5
iPopupY=10

; Language ID
;
iLangID=0

; Treat '0000000' numbers as UNKNOWN.
;  Range: boolean (0 or 1)
;  Default: 0
;
bTreatZeroNumberAsUnknown=0
bProperShutdown=1

[Settings]
MainDlgX=498
MainDlgY=169
CJListPB=185,90,0,0,167,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,267,0,0,0,0,0,
CJListIn=133,0,0,46,94,100,0,0,0,
CJListInboxcx=401
CJListInboxcy=363
sfDate=ddd, MMMM dd
sfTime=HH:mm
bShowMenu=1
Control=170,97,0,
inbox_iPlayTo=0
CJListInboxX=89
CJListInboxY=188
bDockBoxes=1
bConfirmDelete=1
CJListBoxSortCol=0
CJListBoxSortDir=0
CJListBoxColOrder=0,4,5,3,1,2,6,7,8,
CJListPBcx=686
CJListPBcy=494
CJListPBSortCol=0
CJListPBSortDir=1
CJListPBColOrder=0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,
m_bShowTextLabels=1
CJListDialSortCol=0
CJListDialSortDir=0
bStoreInTrash=1
m_bShowTextLabelsInbox=1

