
;   Configuration file for RFM version 1.0

;----------------------------------------------------------------------

; NAMEFILE is the name of the RBBS-PC Fast File Search (FFS) index file
; LOCATIONFILE is the name of the FFS directory list

 NameFile     f:\rbbs\FIDX.DEF
 LocationFile f:\rbbs\LIDX.DEF

;----------------------------------------------------------------------

; WORKPATH specifies a RAM drive or disk with ample free space to use
;          for work files during processing

 WorkPath     f:\source

;----------------------------------------------------------------------

; UPLOAD defines the RBBS-PC upload file area.  In this example, the
;        first character of the file name has been included in the
;        upload specification in order to define different download
;        paths for RFM to move the files into.  The lines given tell
;        RFM to move the files after they have been in the upload area
;        for more than 7 days.  The last UPLOAD entry (without the
;        initial letter of the file name) will pick up the remaining
;        files (those whose names begin with a special character).

 UpLoad       h:\UpLoad\0*.*        7   h:\DownLoad\0
 UpLoad       h:\UpLoad\1*.*        7   h:\DownLoad\1
 UpLoad       h:\UpLoad\2*.*        7   h:\DownLoad\2
 UpLoad       h:\UpLoad\3*.*        7   h:\DownLoad\3
 UpLoad       h:\UpLoad\4*.*        7   h:\DownLoad\4
 UpLoad       h:\UpLoad\5*.*        7   h:\DownLoad\5
 UpLoad       h:\UpLoad\6*.*        7   h:\DownLoad\6
 UpLoad       h:\UpLoad\7*.*        7   h:\DownLoad\7
 UpLoad       h:\UpLoad\8*.*        7   h:\DownLoad\8
 UpLoad       h:\UpLoad\9*.*        7   h:\DownLoad\9
 UpLoad       h:\UpLoad\a*.*        7   h:\DownLoad\a
 UpLoad       h:\UpLoad\b*.*        7   h:\DownLoad\b
 UpLoad       h:\UpLoad\c*.*        7   h:\DownLoad\c
 UpLoad       h:\UpLoad\d*.*        7   h:\DownLoad\d
 UpLoad       h:\UpLoad\e*.*        7   h:\DownLoad\e
 UpLoad       h:\UpLoad\f*.*        7   h:\DownLoad\f
 UpLoad       h:\UpLoad\g*.*        7   h:\DownLoad\g
 UpLoad       h:\UpLoad\h*.*        7   h:\DownLoad\h
 UpLoad       h:\UpLoad\i*.*        7   h:\DownLoad\i
 UpLoad       h:\UpLoad\j*.*        7   h:\DownLoad\j
 UpLoad       h:\UpLoad\k*.*        7   h:\DownLoad\k
 UpLoad       h:\UpLoad\l*.*        7   h:\DownLoad\l
 UpLoad       h:\UpLoad\m*.*        7   h:\DownLoad\m
 UpLoad       h:\UpLoad\n*.*        7   h:\DownLoad\n
 UpLoad       h:\UpLoad\o*.*        7   h:\DownLoad\o
 UpLoad       h:\UpLoad\p*.*        7   h:\DownLoad\p
 UpLoad       h:\UpLoad\q*.*        7   h:\DownLoad\q
 UpLoad       h:\UpLoad\r*.*        7   h:\DownLoad\r
 UpLoad       h:\UpLoad\s*.*        7   h:\DownLoad\s
 UpLoad       h:\UpLoad\t*.*        7   h:\DownLoad\t
 UpLoad       h:\UpLoad\u*.*        7   h:\DownLoad\u
 UpLoad       h:\UpLoad\v*.*        7   h:\DownLoad\v
 UpLoad       h:\UpLoad\w*.*        7   h:\DownLoad\w
 UpLoad       h:\UpLoad\x*.*        7   h:\DownLoad\x
 UpLoad       h:\UpLoad\y*.*        7   h:\DownLoad\y
 UpLoad       h:\UpLoad\z*.*        7   h:\DownLoad\z
 UpLoad       h:\UpLoad\*.*         7   h:\DownLoad\_

;----------------------------------------------------------------------

; FILESPEC defines the download directories.  The /s option tells RFM
;          to scan all subdirectories for the given file specification
;          as well as the directory given.  Files in H:\DOWNLOAD and
;          its subdirectories will be archived if not accessed within
;          180 days.

 FileSpec     h:\SDN\*.*/s
 FileSpec     g:\DVNet\*.*
 FileSpec     h:\RBBS\*.*
 FileSpec     h:\FileList\*.*
 FileSpec     h:\NetFiles\*.*
 FileSpec     h:\DownLoad\*.*/s   180   h:\Archive
 FileSpec     c:\RBBS\Bulletin\Bullet*.

;----------------------------------------------------------------------

; FMSFILE    is the name of the RBBS-PC FMS directory to be verified.
; FMSALPHA   tells RFM to produce an alphabetic FMS directory in addition
;            to the normal date-ordered directory.
; FMSMISSING tells RFM to label directory entries for missing files as
;            "missing".
; FMSCAT     tells RFM to assign category UNC to any files added to the
;            FMS directory.
; FMSDESCLEN tells RFM to write the new FMS directory using 45 character
;            descriptions, no matter what the old directory used.

 FMSFile      f:\rbbs\fms.dir
 FMSAlpha     i:\fmsalpha.dir
 FMSMissing   missing
 FMSCat       unc
 FMSDescLen   45

;----------------------------------------------------------------------

; BULLETIN tells RFM to write the directory entries of download area
;          files that will be archived within the next 30 days to a
;          bulletin file called BULLET50.

 Bulletin     f:\source\Bullet50  30
