11. Select the original 2D profile you created in Step 8 and press [command] E to bring up the Extrude dialogue box. Select the Straight extrusion profile, and type 1.0 into the Depth field. Click OK to extrude. Repeat Steps 8 and 9 with this object, centring each of them on their respective engine housings.