UUCP Information

Wrap Length - This is the length that CP will use to force a hard <CR> into an outbound messages.  UUCP/Wrap option has to been checked under the each area for this to become operational.  This is mainly used to provide complience for Internet outbound messages.

UUCP Gate:  This is the address of the fidonet gateway, that you will passing your internet messages through.  Example:  226/20

Freq Cmd:  This is the default FREQ command used with file requesting via the internet.  Default: $MACARCH GET 

'To' Default - This is the default UUCP address for the site where request are directed to.  Default: To: LISTSERV@ricevm1.rice.edu

Save Button - Will save the information is the current dialog box as new default information.

Cancel Button - will revert to the old setting, as they were prior to enter this dialog box.