Custom Echo Data

Custom Echo packets may be constructed by selecting Custom Echo or Custom ICMP Echo from the Probe Type pop-up menu. The values entered become the data of the AppleTalk or ICMP Echo packet. The data may be entered in either hexadecimal or ASCII. The length of the data  (in bytes) is shown in the lower left corner.