NAME

cdrecord –

SYNOPSIS

cdrecord [ ] dev=device [ ] track1 trackn

DESCRIPTION Cdrecord

The device scsibus/target/lun SunOS scg.

dev= scsibus,target,lun or dev= target,lun Scsibus, target and lun

dev= devicename:scsibus,target dev= devicename:target,lun dev= devicename:@ or dev= devicename:@,lun dev= devicename:scsibus,target,

cdrecord UNIX dev= devicename:scsibus,target

scsibus,target,lun.

Scsibus

/var/adm/messages scsibus,target,lun –scanbus cdrecord

dev=

On SVr4 cdrecord

In track – stdin.

–version –v –V –VV –V or –VV

–debug –debug

–force

–dummy

–dao Set mode.

–multi

. The Sony –data CD-ROM sec- –data

–msinfo mkisofs-1.10

–toc cdrecord will

–atip cdrecord

If cdrecord –fix

–nofix

–waiti cdrecord mkisofs cdrecord opens

–load

–eject – speed=# #. #

speed cdrecord CDR_SPEED speed=2 or speed=4 speed=0.

blank= type

gap.

–force blank= all cdecord –force

fs=# # dd(1), sdd star ∗ ∗ fs=10x63k

fs= fs cdrecord CDR_FIFOSIZE

from mkisofs cdrecord mkisofs into cdrecord cdrecord if mkisofs dev=target dev=6,0 FreeBSD CAM sup- /dev/rcd0.ctl dev=/dev/rcd0.ctl:@ .

dev cdrecord CDR_DEVICE environment. dev= @ timeout= # #

timeout driver= name driver=help cdrecord with cdrecord –speed or –dummy

cdr_simul and dvd_simul –dummy CDR_SIMUL_BUFSIZE –dummy driveropts= driveropts= help –checkdrive burnproof

–checkdrive cdrecord –prcap kB KB

–inq –scanbus

bus ∗ –reset

systems. –ignsize

–useinfo

Use ∗ ∗ defpregap =#

–packet Set pktsize=# # –noclose

mcn=med _cat_nr med_cat_nr.

isrc=ISRC _number ISRC_number.

index=list

–audio CD-DA

.au or .wav Cdrecord

–pad cdrecord recog-

Cdrecord will

cdrecord

–data nor –audio cdrecord –audio .au or .wav –data –swab

Cdrecord

–swab

cdrecord Cdrecord –swab –data ISO- 9660 or mkisofs ufs

– –data nor –audio cdrecord –audio .au or .wav –data –mode2

–xa1

–xa2

–cdi CDI

–isosize ISO-9660

–isosize –isosize cdrecord cdrecord stdin

–pad –pad padsize= padsize=15s. –pad track, cdrecord

–pad –nopad .

padsize=# # –pad padsize= fs Linux

–nopad – pregap =#

–preemp

–nopreemp – tsize=#

–isosize

cdrecord

tsize of cdrecord . See fs

EXAMPLES

cdimage.raw:

cdrecord – mkisofs – R –

mount – r – –

– r – –

ls –

mkisofs – cdrecord – fs= mkisofs command

mkisofs – by priocntl – e – – –

–

track01.cdaudio, track02.cdaudio cdrecord – ∗.cdaudio

cdrecord – v – – ∗.cdaudio cdimage.raw track01.cdaudio, track02.cdaudio cdrecord – v – – ∗.cdaudio where XXX

∗.wav ENVIRONMENT CDR_DEVICE

CDR_SPEED –speed option).

CDR_FIFOSIZE fs=# option).

FILES

/etc/default/cdrecord

CDR_FIFOSIZE=8m or CDR_SPEED=2 CDR_DEVICE

CDR_SPEED –speed option).

CDR_FIFOSIZE fs=# option).

@

for speed and fifosize

cdrecord teac1

mkisofs(1), scg(7), fbk(7).

NOTES

Cdrecord

session.

–dummy cdrecord NFS cdrecord NFS cdrecord with

Cdrecord /dev/scg?

cdrecord

use cdrecord, enter:

cdburners

/dev/scg?

http://www.hp.com/isgsupport/cdr/index.html

cdrecord cdrecord uses Linux

Cdrecord

Cdrecord count.

Cdrecord >

DIAGNOSTICS ^ cdrecord

fatal error copy

scsierrs.c

BUGS

Cdrecord ls. Cdrecord

CREDITS _Swartz@twolf.com) @wdc.com) @andante.jic.com) @netvision.net.il) @guardian.no) @feghoot.ml.org) cdrecord.

@eng.us.uu.net)

@torque.net) @kdm.org)

(msmith@freebsd.org)

other-cdwrite-request@lists.debian.org subscribe cdwrite@lists.debian.org AUTHOR J

Germany http://www.fokus.gmd.de/usr/schilling/cdrecord.html

joerg@schily.isdn.cs.tu-berlin.de or js@cs.tu-berlin.de or schilling@fokus.gmd.de