2. Install the batteries noting carefully the correct (+) and (-)  positions. (Fig. 2).