Operation Instructions 

To extend the detector, release the locking tab, extend to desired length and lock tab. (Figure 7) 

Search Methods 
l.Sweep the loop close and parallel to the ground. 
(Figure 8 & 9)