3. Close battery compartment in a clockwise direction. (Fig. 3)