USE OF THE VIEWER1. Loosen the screw under the eyepiece in counterclockwise direction. Replace the eyepiece with the viewer and tighten the screw. To increase the brightness of the image, cover fihe Illuminator Lamp with Condenser Lens Cap (provided in the set).
2. NEVER USE THE CONDENSER LENS CAP WHEN YOU ARE LOOKING THROUGH THE EYEPIECE. Insert the plastic viewer screen into the slot on top and lip the reflective mirror (as shown in the picture abovej
Carefully put prepared slide on the stage and beneath the clips. Adjust the positions of the slide and the illuminator such that the largest amount oF light goes through the stage hole onto the objective lens. While moving the body tube by the focusing knob, look at the viewer screen to check for a clear projection of the sample. If the image on the screen is too dark, adjust the light source lamp, which should not be turned over 180¡.
3. Observation of the sample can be made without interruption for about an hour, due to the life time of battery . When the microscope is not used, turn off he illuminator lamp by Hipping the mirror side upward.