Search Methods 

2.The loop must be in continuous motion (moving from side to side) in order for the detector to respond to metals. If the loop is held stationary, the detector.may not respond. (Figure 10).

3.Where metal is located, a "BEEP" tone will be heard and the "RED" LED is on. (Figure 11 ).

Detection .Ranges (approximate)
For Ring 			30 mm  
For Key 			40 mm 
For Watch  			50 mm 
For Gun 			120 mm 
For 6 Inch Dagger 	150 mm