Insert three 1.5V sice "C" batteries into the battery compartment.