- Load Menu Commands         
           LOAD MENU COMMANDS

• Download user program…
Download a EZ-KIT Lite memory image file (*.exe).

• Download and execute…
Download a EZ-KIT Lite memory image file (*.exe) and execute it from it's entry address. (the entry address is the first location of the program memory image kernel).

• Upload data memory…
This command uploads a block of DSP data memory content to a memory image (*.exe) file on the host computer. Specify in hexadecimal the starting address and number of words.

• Upload program memory…
This command uploads a block of DSP program memory content to a memory image (*.exe) file on the host computer. Specify in hexadecimal the starting address and number of words.

• Download data memory…
This command downloads a memory image (*.exe) file from the host computer into DSP data memory.

• Download program memory…
This command downloads a memory image (*.exe) file from the host computer into DSP program memory.