		;*]------------------------------------[*]
		 ;					|
		 ;		NETLIST.DEF		|
		 ;	   NETLIST defaults file	|
		 ;					|
		;*]------------------------------------[*]

/N	# Hash-out this line to make NETLIST use
	# this default configuration file.

# The longer this file, the more time NETLIST will need to start.
# #'s and ;'s void the rest of their line.

#/A NETLIST.LOG	# Archive the results in NETLIST.LOG (current directory).
		# You can specify a full path to put the log elsewhere.
# /B 10		# At most 10 simultaneous polls at once
# /D		# Debug mode: display all names defined by adapters
# /E		# Display possible NetBIOS error replies.
/F		# Perform a namefile search, if no other general argument.
# /H		# Display help. /? can also be used.
/I		# Interactive update. NETLIST will ask for remarks.
# /L		# Wait after search/scan/test completion
# /M		# Enter monitor mode: clear screen, display tx/rx packets.
# /N		# Do not use the settings from this file.
# /P HexIntNo	# Use this interrupt rather than the default 0x5C or 0x2A.
# /R		# Repeat the test continuously. /M can be useful.
# /s \id1 \id2	# Scan a range of adapter numbers.
/t1		# Answer timeout is 1 clock tick.
/U		# Update the database at the end.
/X		# Display all names found on adapters.
