.7 Parameter  "Fax"

All pre-settings necessary for the fax service can be edited in this dialogue box.

Fax-Speed

At this field select the highest transmission speed available to your modem. Once connection has taken place the programme allows connection between machines at an agreed speed. The highest speed will obviously be restricted to what your modems will support. Normally you will have to work down when connecting to pure fax. But this works automaticaly in CoMa!

Zoom 50%

You select the zoom factor with which a fax page is displayed after loading. You can change display with the keys "+" and "-" of the number block at any time.

ID (send identification)

Enter your telephone number in this field.  Every fax will carry this number in the stampline (first line of a fax page) next to your name.

      standard fax-resolution

In this pop-up-menue you set the default fax-resolution. Whenever you send a fax you can change to a different resolution if needed. Befor sending the fax you are asked what resolution. If you want to use the default setting just do nothing and go on sending the fax.

 

Path for a polling folder "send Poll"

This function works only in CoMa professional!

Modems can answer a poll request from modem standard class 2.0 (not to be confused with class 2) and send fax pages to the caller. The calling modems sends a certain tone for this which can only be understood from modem class 2.0 onwards. 

You can store fax pages for transmission in Hufman format in a folder for this.

Send at poll request

The command "send at poll request" below this path activates and de-activates this function. This button must be activated to allow polling to take place.

Receive max. A4 page
 
This function tells the modem that a page of only 29,5 cm should be received. Unfortunately fax machines do not comply with this request.

online screen redraw 

If you activate this button the fax page will be displayed immediately it is received, in a window. This means you will not have to leave the programme to read the fax. The displayed fax can be moved to enable you to read the whole page via the mouse.

last line for error line 

Quite often during transmission, and particularly reception from older fax machines, a lot of errorneous data is imported. This tends to make the readability worse and also uses up a lot of memory on reception. By activating this box the fax can be cleaned up by ignoring these errors. It is not a perfect system and you should use trial and error to see which suits you best. Once you have made your adjustments in this sector do not forget to save them by activating the button "save parameter" otherwise all changes will be lost.

         print immediatly after receive

If you activate this function every faxpage is printed after receiving it. This will cost you a lot of paper. You should choose the important fax pages by hand and print only these!