.4 Select button "Send Fax..."

The "Send" button is nearly the final input stage for a fax transmission. 

A last box askes for the folder and the desired resolution of the transmission.

100/200 dpi

You can switch between the low resolution and the high fax resolution. If you work with 100 dpi you spare time and telephone costs.

+Pages in Folder 

With this function you can sent a hole folder with fax pages without loading the pages into preview windows. Every opend preview window will be sent together with the pages in the folder. For details see next chapter.

Logbook-File 

After every transmission CoMa writes a logbook file.

If you want to know the transmission speed, time of transmission etc. after a transmission you can call up the required logbook entries with a double click on the relevant line of the calls-list and read/print them. 

Have you sent a top page you can see what header/footer you had used and the text you had written.

More than one entry can be selected and exported into a text file and so more than one entry can be printed together.

Once selected the modem will go "off hook", dial and automatically negotiate connection parameters with the other side. The comment line will show transmission speed, resolution and the other side's ID (i.e. telephone number). There is no delay time for the fax to be encoded and transmitted. 

Any error messages to do with fax selection will appear prior to the modem going "off hook", any transmission errors will be shown in the comment line after transmission.

CoMa has got no influence over the quantity and the quality of transmission error messages. It only reports error messages from the modem. Unfortunately there are quite a number of modems in existence that do not report error messages at all.

After pressing the "Send Fax..." button you see another dialog box. Here you can make the relevant settings for this fax transmission.