.10 "Dial Voice No.", the dial automat

This function is nearly self explanatory. You can use your modem as dial automat. Activate the required telephone number with a click and select the command "Dial Voice no" from the pop-up-menue "Function in the number-list" and your modem starts to dial. CoMa passes on the number from the entry in the field "Telephone number". You can start the function with the key combination âŒ˜ + D as well.

You can start dialing also by clicking on the button "Dial Voice" in the main dialoque-box.

The telephone has to be connected to the same telephone socket for you to be able to take over the call.

If the connection answers you can force the modem to hang up by pressing the keys âŒ˜ +"."  or the Esc key. The call will then be transferred to the connected telephone and you can start speaking.