BEGIN DDIF

-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Digitizing Tablets using a 5 or 6      --
--                          byte packed bimary format                  --
--                                                                     --
-------------------------------------------------------------------------

--
-- 7-2-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

--- Input Device Driver ---

--    +-- Digitizer input wait loop counter
--    |  +-- Number of digitizer units to consider as a cursor change
--    |  |     (Increase this number if the cursor 'jiggles' on the screen)
--    |  | +-- Digitizer number of push buttons to validate PB
--    |  | | +-- Digitizer number of buttons on stylus
--    |  | | |   +-- Digitizer units per inch (resolution)
--    |  | | |   |    (Normally 200 = 5 byte format, 1000 = 6 byte format)
--    |  | | |   |   +----+-- Digitizer X,Y active area in digitizer units
--    |  | | |   |   |    |     (Active area for tablet menu)
--    |  | | |   |   |    |    +-- Digitizer RTS flag
--    |  | | |   |   |    |    |  +-- Digitizer 5/6 byte format
--    |  | | |   |   |    |    |  |     (6 byte format returns 4 byte coords)
--    |  | | |   |   |    |    |  |     (5 byte format returns 2 byte coords)
--    |  | | |   |   |    |    |  |  +-- COM port to use (1 or 2)
--    |  | | |   |   |    |    |  |  |  + PARITY (0=disable,1=odd)
--    V  V V V   V   V    V    V  V  V  V
101 800  1 2 1 200 2200 2200   1  5  1  0

END DDIF
END

