BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Hewlett-Packard 7470A plotter (A size) --
--                                                                     --
--                                                                     --
-------------------------------------------------------------------------
-- 10-15-89 JSM Added prefix & suffix string, port information, etc.
-- 7-17-87 TT - Set COM1 as release port
-- 7-06-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 1  -- communications port number:
--  0 = custom port configuration, see documentation for more information
--  1 = COM1
--  2 = COM2
-- -1 = LPT1 (using BIOS) \
-- -2 = LPT2 (using BIOS)  - these can be redirected by most networks
-- -3 = LPT3 (using BIOS) /  (10k bits per second)
-- -4 = LPT1 (using direct I/O) \
-- -5 = LPT1 (using direct I/O) - These are very fast, but do not work
--                                on all machines, and cannot be redirected
--                                by any networks
--                                (80k bits per second)
   
1  'A A4 AY  '   -- Paper size string (must have space at end)
105 0 0  1       -- XY axis rotation flag for each paper size

-- Paper sizes
201  0       0   10300    7650  -- A size
202  0       0   10900    7650  -- A4 size
203  0       0    7650   10400  -- AY size

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  2  1 1

--    +-----+------ X,Y plotter units per inch
--    V     V
103 1010  1010

104 38           -- Max pen speed

-- Prefix string to sent before plot (use to setup plotter, switches, etc)
--29  ''
-- Suffix string to be sent after plot
--30  ''

END DDIF
END
