BEGIN DDIF
----------------------------------------------------------
-- 4D Graphics TiGA DEVICE INFORMATION FILE             --
-- 12/15/89                                             --
----------------------------------------------------------

-- WIREFRAME COLOR definitions
-- RGB color table values for first 16 colors (for GCD) (range: 0 to F)
1 "000 800 080 008 880 088 808 888 333 F00 0F0 00F FF0 0FF F0F FFF"

-- SHADING COLOR definitions
-- Starting RGB values for the shading color table (range: 0 to F)
2 "888 F00 0F0 00F FF0 0FF F0F 888"

-- RGB increments for the dark shades of each color (range: 0 to F)
3 "888 E00 0E0 00E EE0 0EE E0E 888"

-- RGB increments for the light shades of each color (range: 0 to F)
4 "888 0EE E0E EE0 00E E00 0E0 777"

-- Beep definition line in duration,frequency divisor pairs
-- (divisor = 1193180/desired freq, ie divisor for 400hz = 2983)
-- Up to 10 pairs may be given.
-- This line is optional and may be commented out to get the default beep.
102 8 4200 4 3800 2 3400 2 3000 2 2600 2 2200 2 1800 8 1400 4 1000 4 800

-- Custom features:
--  
--  +-- load TiGA primatives in initialization (revision 4.0 only)
--  |  +-- TiGA mode number
--  |  |  +-- beep mode: 0 = sound only, 1 = sound and flash, 2 = flash only
--  |  |  |  +-- text alignment code (normally 1) custom fonts may be "0"
--  |  |  |  |  +-- restore screen clipping flag (1=whole screen, 0=window)
--  |  |  |  |  |  +-- maximum number of words to pass via putlinbuf (rev 4.0)
--  |  |  |  |  |  |   +-- pixel width for menu hilighting (0 = fill)
--  |  |  |  |  |  |   |  +-- Two screen configuration (1=yes, 0=no)
--  v  v  v  v  v  v   v  v
103 1  0  1  1  1  512 0  0

-- name of custom text font to use instead of hardware text
--5 "ti_typ22.fnt"

-- Up to 8 32-BIT text font patterns
201 -1431655766 -858993460 -252645136 -242224753 
202 -429398425 -473489864 -522133280 858993459


-- PIXEL DENSITIES (you must set these for your monitor)
-- for most 13" monitors, pixels in x dimension would be xres/8.5
--                        pixels in y dimension would be yres/6.375
--    +-----+-- X,Y SCREEN PIXELS/PER INCH
--    V     V
--301 63.77 50.24         -- 640x480 on 13" monitor
301 90.62 92.53         -- 1024x768 on 16" monitor

--   GRAPHICS DRIVER CONFIG FLAGS.
--  *** DO NOT CHANGE THIS LINE ***
--  0 in a line number field means not used.
--    +-------------------------------- 0 = low res   ,  1 = high res.
--    |    +--------------------------- Color lookup table line number
--    |    |    +---------------------- Start shade color table line number
--    |    |    |    +----------------- Dark shade color table line number
--    |    |    |    |    +------------ Light shade color table line number
--    |    |    |    |    |    +------- Number of dsplist 16k's line number
--    |    |    |    |    |    |    +-- Dsplist o/f file name line number
--    |    |    |    |    |    |    |
120   1    1    2    3    4    0    0

END DDIF

END


