Aliased, 1-bit images are used while the globe is in motion.