±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±

1	Submitted:	Juergen Moellenhoff	Aug 19 1997 00:00
	Topic:		/PPP-2.3/Kernel Server/Panic/
	Status: 	New Bug
	Severity:	System Hang/Crash
	Priority:	Unknown
	
	Kernel Panic after PPP link started
	
[jurgen@oic.de Sun Aug 17 19:51:19 CDT 1997]
Hi,

I tried to use PPP-2.3b3 (for NeXT) on a OpenStep 4.2 for Intel system and got a kernel Panic after the PPP link started. I compiled the version on a NEXTSTEP 3.3 system with _no optimization_ turned on, but I got the problem _with optimization_, too. This is the output of hostconfig:

----------------------------------------------------
Mach kernel version:
         NeXT Mach 4.2: Wed Apr 16 13:44:57 PDT 1997; root(rcbuilder):Objects/mk-183.34.obj~2/RELEASE_I386

Kernel configured for a single processor only.
1 processor is physically available.
Processor type: I386 (Intel 586)
Processor active: 0
Primary memory available: 96.00 megabytes.
Default processor set: 86 tasks, 171 threads, 1 processors
Load average: 1.00, Mach factor: 0.00
----------------------------------------------------

The last output in the Monitor window was:

-------------------------------------
Memory access exception (1, 1, c617fffc)
-------------------------------------

Sorry, that's all.

Bye,

	Juergen Moellenhoff

±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±