–	Continuous service -70°F to +475°F