•	Last three times longer than high-temp phenolic wheels