•	Low heat build-up in continuous tow-line applications