•	Superior resistance to chipping, cracking and flat-spotting