BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Hewlett-Packard 7475A plotter (B size) --
--                                                                     --
--                                                                     --
-------------------------------------------------------------------------
-- 10-15-89 JSM Added prefix & suffix string, port information, etc.
-- 05-31-88 KMM - Added metric paper size
-- 07-17-87 TT  - Set COM1 as release port
-- 07-06-87 TT  - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

101 1  -- communications port number:
--  0 = custom port configuration, see documentation for more information
--  1 = COM1
--  2 = COM2
-- -1 = LPT1 (using BIOS) \
-- -2 = LPT2 (using BIOS)  - these can be redirected by most networks
-- -3 = LPT3 (using BIOS) /  (10k bits per second)
-- -4 = LPT1 (using direct I/O) \
-- -5 = LPT1 (using direct I/O) - These are very fast, but do not work
--                                on all machines, and cannot be redirected
--                                by any networks
--                                (80k bits per second)
   

1  'B A AY BS A4 A3 '  -- Paper size string (must have space at end)
105 0 0 1  0  0  0  -- XY axis rotation flag for each paper size

-- Paper sizes
201  0       0    16640    10365   -- B size
202  0       0    10365     7962   -- A size
203  0       0     7962    10365   -- AY size
204  0       0    16140    10365   -- BS size
205  0       0    11104     7721   -- A4 size
206  0       0    16158     11040  -- A3 size

--  +--+----------- Smallest, largest pen numbers
--  |  |  +-------- Do pen changing optimization  { good for plotters, }
--  |  |  | +------ Do pen movement optimization  { bad for printers!  }
--  V  V  V V
102 1  6  1 1

--    +-----+------ X,Y plotter units per inch
--    V     V
103 1021  1021

104 38           -- Max pen speed

-- Prefix string to sent before plot (use to setup plotter, switches, etc)
--29  ''
-- Suffix string to be sent after plot
--30  ''

END DDIF
END
