BEGIN DDIF
-------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  for Pixelworks Clipper High Resolution     --
--                          display controller board                   --
--                                                                     --
-------------------------------------------------------------------------
-- 10-16-89 JSM Incorporated Pixelworks' and 4D's latest changes
-- 06-15-88 ALA Fix aspect ratio [for PCClient].
-- 01/12/88 NCC Added code line 6 for display list overflow file name
-- 7-27-87 NCC  Upgraded further for rev 3.0 and 3.10
-- 6-24-87 TT - Upgraded for rev 3.0
------------------------------------------------------------------------
-- ******** Attention all programmers: you must document any ******** --
-- ******** and all changes you make to this file at the top! ******* --
------------------------------------------------------------------------

-- Graphics Device Driver --

-- The file name to echo commands to is given on code line 1.  To activate
-- this feature remove the '--' comment characters in front of the 1 or put 
-- in a '--' to deactivate it.  The file can then be displayed by copying it
-- to the CGB device. Ie. C>COPY /B PW.CGB CGB:

--1 PW.CGB

-- Color Table Definition

--    +---Index 0 is the graphics background color (000 = black)
--    |
--    |                 Entity Color Table
--    |                 ------ ----- -----
--    |                 Color Table Values (RGB) (0-9)(A-F)
--    |                 (0 - 9 & A   0 = Dimmest, A = Brightest)
--    V
--    0   1   2   3   4   5   6   7   8   9  10  11  12  13  14  15
--    +---+---+---+---+---+---+---+---+---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |   |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V   V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB RGB 
2   "100 500 050 005 640 058 505 666 000 800 080 008 870 07A 808 999"

--          Starting Shading Color Table Values (RGB)
--          -------- ------- ----- ----- ------ -----
--    0   1   2   3   4   5   6   7   
--    +---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB
--3   "000 800 080 008 880 088 808 000"
3   "000 808 080 088 088 080 800 800"

--                Dark Shading Color Increments (RGB)
--                ---- ------- ----- ---------- -----
--    0   1   2   3   4   5   6   7
--    +---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB
4   "111 100 010 001 110 011 101 111"

--               Light Shading Color Increments (RGB)
--               ----- ------- ----- ---------- -----
--    0   1   2   3   4   5   6   7
--    +---+---+---+---+---+---+---+
--    |   |   |   |   |   |   |   |
--    V   V   V   V   V   V   V   V
--   RGB RGB RGB RGB RGB RGB RGB RGB
5   "111 011 101 110 001 100 010 111"


--  +-- Cursor character number
--  V
101 95

-- 16 bit line font patterns           (Entity ident hilite font)
--                                                  |
--                                                  V
--    1     2    3      4      5      6      7      8
102 6168  4080  8184  32742  32663  15420    15   26214

-- Beep definition line in duration,frequency divisor pairs
-- (divisor = 1193180/desired freq, ie divisor for 400hz = 2983)
--
-- Up to 10 pairs may be given.
-- This line is optional and may be commented out to get the default beep.

103 4 4200 2 3800 1 3400 1 3000 1 2600 1 2200 1 1800 4 1400 2 1000 2 800

-- The number on line 109 is for how many 16-k pages of Expanded Memory
-- to allocate for saving a display list in.

109 0  --number of 16k pages to allocate for display list (32 = 512k bytes)

6 display.ovl            --display list overflow file name

--    +-----+-- X,Y Screen pixels per inch
--    V     V
--301 94.4 96.8
301 94.4 100.69

--Custom configuration options
--110 6           --DMA Channel to use with Clipper (6 or 7)
--111 10          --IRQ Vector to use with Clipper (10, 11 or 12)
--112 816         --I/O Ports to use with Clipper (816 or 832)
--113 0           --Flag to Enable Page Swapping (-1=yes)

-- For Ultra clipper only:
-- 16 bit line font patterns           (Entity ident hilite font)
--                                                  |
--                                                  V
--    1     2    3      4      5      6      7      8
--114 6168  4080  8184  32742  32663  15420    15   26214

END DDIF
END
