BEGIN DDIF
------------------------------------------------------------------------
-- DEVICE INFORMATION FILE  FOR DIGITIZING TABLETS USING 5 OR 6 BYTE
--                              PACKED BINARY FORMAT
-- 05/03/88  ALA  Add the parity flag.
-- 09/01/87  KMM  Created
------------------------------------------------------------------------

-- INPUT DEVICE DRIVER ----------------------------------------------

--     +-- DIGITIZER INPUT WAIT LOOP COUNTER
--     |  +-- DIGITIZER DELTA UNITS TO BE CONSIDER AS CHANGED
--     |  | +-- DIGITIZER NUMBER OF PUSH BUTTONS TO VALIDATE PB
--     |  | | +-- DIGITIZER NUMBER OF BUTTONS ON STYLUS
--     |  | | |    +-- DIGITIZER UNITS PER INCH (RESOLUTION)
--     |  | | |    |    +-----+-- DIGITIZER X,Y ACTIVE AREA IN DIGITIZER UNITS
--     |  | | |    |    |     |            divided by 2
--     |  | | |    |    |     |     +-- DIGITIZER RTS FLAG
--     |  | | |    |    |     |     |  +-- DIGITIZER 5/6 BYTE FORMAT
--     |  | | |    |    |     |     |  |  + COMPORT TO USE(1 or 2)
--     |  | | |    |    |     |     |  |  |  + ODD PARITY (0=disable,1=enable)
--     V  V V V    V    V     V     V  V  V  V
101 4000 10 2 1  1000 12000 12000   1  5  1  0

END DDIF
END

