InS_StArT
CNWODI.COM
1.0,CNWCFG.EXE
^Xircom CreditCard NetWave Adapter,CNWODI.COM,IEM
?Installation for the Xircom CreditCard NetWave Adapter.
!$OIEM(INT) Hardware Interrupt
?The default hardware interrupt is 5.
3  
4
@5
6
7
8
9
10
11
12
13
14
15
!$OIEM(PORT) Base I/O Port Address
?The default base I/O port address value is 300.
240
260
280
2A0
2C0
2E0
@300
320
340
360
380
$OIEM(MEM) Memory I/O Address
?The default memory I/O address value is D0000.
C0000
E8000
@D0000
$OIEM(DOMAIN) Domain
?The default domain is 100.  The domain is a hex number.  Use 000-0ff if no access point is going to be used, and 100-1ff if an access point is going to be used.
000
1ff
@100
*OIEM(FRAME) Frame type
?The latest ODI Specification uses Ethernet_802.2 as the default frame type.  If your network requires something other than Ethernet_802.2, then make sure to specify the correct frame type.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIEM(IOWORDSIZE) I/O Word Size
?The default is to not specify I/O word size.
8
!OIEM(MODE) MODE
?The default is to not specify the MODE keyword.
IO
!$OIEM(SOCKETSERVICES) Socket Services
?The default value is Y.  Select N if you know the Socket Services available on your system does not comply with the PCMCIA Specification.  Choosing N forces the Xircom CreditCard to ignore Socket Services and interface directly to the PCMCIA hardware.
@Y
N
!$OIEM(CARDSERVICES) Card Services
?The default value is Y.  Select N if you know the Card Services available on your system does not comply with the PCMCIA Specification.  Choosing N forces the Xircom CreditCard to ignore Card Services and interface directly to the PCMCIA hardware.
@Y
N
$OIEM(SCRAMBLEKEY) SCRAMBLEKEY
?The default is to not specify a value.
0
65535
InS_EnD
