InS_StArT
CEODI.COM
1.0,CECFG.EXE
^Xircom CreditCard Ethernet Adapter,CEODI.COM,IEM
?Installation for the Xircom CreditCard Ethernet Adapter.
!OIEM(INT) Hardware Interrupt
?The default hardware interrupt is 5.
3  
4
@5
6
7
8
9
10
11
12
13
14
15
!OIEM(PORT) Base I/O Port Address
?The default base I/O port address value is 300.
240
260
280
2A0
2C0
2E0
@300
320
340
360
380
$OIEM(MEM) Memory I/O Address
?The default memory I/O address value is D0000.
C0000
E8000
*OIEM(FRAME) Frame type
?The latest ODI Specification uses Ethernet_802.2 as the default frame type.  If your network requires something other than Ethernet_802.2, then make sure to specify the correct frame type.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIEM(SOCKET) Socket
?The default socket value is 1.
@1
2
!OIEM(IOWORDSIZE) I/O Word Size
?The default I/O word size is 16.
8
@16
!OIEM(SOCKETSERVICES) Socket Services
?The default value is Y.  Select N if you know the Socket Services available on your system does not comply with the PCMCIA Specification.  Choosing N forces the Xircom CreditCard to ignore Socket Services and interface directly to the PCMCIA hardware.
@Y
N
!OIEM(CARDSERVICES) Card Services
?The default value is Y.  Select N if you know the Card Services available on your system does not comply with the PCMCIA Specification.  Choosing N forces the Xircom CreditCard to ignore Card Services and interface directly to the PCMCIA hardware.
@Y
N
!OIEM() Link Integrity Disabling
?Select the LINKDISABLE keyword only if you wish to disable link integrity checking.
LINKDISABLE
InS_EnD
