;reverb def file (c)2001 NovaLogic, Inc.
;note - L & R is swapped with every bounce for stereo echo effect
;       each bounce includes a 6db filter at 11KHz
;       prefered send is amplitude, -amplitude/4
;       this gives a nice rear stereo bounce echo with the L/R swap
;
;       since the channels are swapped, the echo equation is as follows:
;       echoL = e1AL*sendL(e1d) + e1AL*e1AR*sendR(e1d*2) + ....
;
;20 reverbs supported #0 to #19

;reverb #0      ;default - outside reverb
0,0           ;primary send L/R levels (-127 to 127, negate for surround)
50             ;echo delay 1 (180ms max)
48,48           ;(L/R, even/odd bounce) amplitude of echo 1 (-127 to 127)
63             ;echo delay 2 (180ms max)
64,64           ;(L/R, even/odd bounce) amplitude of echo 2 (-127 to 127)

;reverb #1      ;Nightclub - Medium
100,-25         ;primary send L/R levels (-127 to 127, negate for surround)
55              ;echo delay 1 (180ms max)
64,64           ;(L/R, even/odd bounce) amplitude of echo 1 (-127 to 127)
110             ;echo delay 2 (180ms max)
32,32           ;(L/R, even/odd bounce) amplitude of echo 2 (-127 to 127)

;reverb #2      ;Sewer Pipe - Small & Big Echo
-25,100         ;primary send L/R levels (-127 to 127, negate for surround)
30              ;echo delay 1 (180ms max)
60,60           ;(L/R, even/odd bounce) amplitude of echo 1 (-127 to 127)
160             ;echo delay 2 (180ms max)
20,20           ;(L/R, even/odd bounce) amplitude of echo 2 (-127 to 127)

;reverb #3      ;Giant Environment
127,-32         ;primary send L/R levels (-127 to 127, negate for surround)
80              ;echo delay 1 (180ms max)
64,-64          ;(L/R, even/odd bounce) amplitude of echo 1 (-127 to 127)
120             ;echo delay 2 (180ms max)
48,48           ;(L/R, even/odd bounce) amplitude of echo 2 (-127 to 127)


< end of reverb (max is reverb #19)
