InS_StArT
EXOS.COM
1.0
^Novell/Excelan EXOS 205T Ethernet,EXOS.COM,IE0
^Novell/Excelan EXOS 215 Ethernet,EXOS.COM,00M,6205
?Please select the options that match your board's jumper settings.
!RIE0(INT)Hardware Interrupt
2
3
4
5
6
7
@9
!R00M(INT)Interrupt
@5
9
10
11
12
14
15
!RIE0(PORT)Base I/O Port
300
@310
320
330
!R00M(PORT)Base I/O Port
300
308
@310
!RIEM(MEM)Base Memory
C0000
C4000
C8000
@CC000
D0000
D4000
D8000
DC000
!R00M(SLOT)Slot
1
2
3
4
5
6
7
8
$OIEM(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIEM(FRAME)Frame Type
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@ETHERNET_802.2
ETHERNET_802.3
ETHERNET_II
ETHERNET_SNAP
InS_EnD
