InS_StArT
3C501.COM
1.0
^3Com 3C501 EtherLink,3C501.COM,IE0
!RIE0(INT)Hardware Interrupt
?You must select the option that matches your board's IRQ jumper setting.
2
@3
4
5
6
7
!RIE0(PORT)Base I/O Port
?You must select the option that matches your board's I/O jumper setting.
200
210
220
230
240
250
260
270
280
290
2A0
2B0
2C0
2D0
2E0
2F0
@300
310
320
330
340
350
360
370
380
390
3A0
3B0
3C0
3D0
3E0
3F0
*RIE0(FRAME)Frame Type
?Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
