InS_StArT
3C503.COM
1.0
^3Com 3C503 EtherLink II,3C503.COM,IE0
^3Com 3C503 EtherLink II TP,3C503.COM,IE0
^3Com 3C503 EtherLink II/16,3C503.COM,IE0
^3Com 3C503 EtherLink II/16 TP,3C503.COM,IE0
?The shared memory or PIO mode can be selected only by the board's memory jumper setting.
!RIE0 (INT) Hardware Interrupt
?Assign a unique interrupt level for the 3C503 LAN board.
2
@3
4
5
!RIE0 (PORT) Base I/O Port
?Select the option that matches your board's I/O jumper setting.
250
280
2A0
2E0
@300
310
330
350
*RIE0 (FRAME) Frame Type
?Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
