InS_StArT
3C523.COM
1.0
^3Com EtherLink/MC,3C523.COM,00M,6042
^3Com EtherLink/MC TP,3C523.COM,00M,6042

?The interrupt, I/O port, and shared memory can be set only with the Micro Channel Setup utility.
!O00M (SLOT) Slot Number
?For multiple adapters, the slot number is required.  This number must correspond to the slot holding the card. 
1
2
3
4
5
6
7
8
*R00M (FRAME) Frame Type
?Note: Ethernet_802.2 is now the default type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
