InS_StArT
T20ODI.COM
1.0
^Cabletron Systems Token-Ring T20,T20ODI.COM,IE0
?Select the options you will use.
!RIE0(DMA) DMA
@5
6
7
!RIE0(INT) Hardware Interrupt
@3
4
5
6
7
9
10
11
12
14
15
!RIE0(PORT) Base I/O Port
@A20
A80
1A20
1A80
!RIE0(MEDIA) Media Port
?Select the media port you will use. Primary: top media port; Secondary: bottom media port.
@PRIMARY
SECONDARY
!RIE0(LINE SPEED) Line Speed
?Select the line speed of the token-ring network, (4 or 16 Mbps).
4
@16
!OIE0(SOURCE ROUTING) Source Routing
?The Cabletron token-ring drivers have built-in source routing abilities.  Use either the built-in source routing abilities or ROUTE.COM.
@OFF
ON
$OIE0(NODE ADDRESS) Node Address
400000000000
7FFFFFFFFFFF
*RIE0(FRAME) Frame Type
@TOKEN-RING
TOKEN-RING_SNAP
InS_EnD
