InS_StArT
TCTOKSH.COM
1.0
^Thomas-Conrad TC4035/TC4045 adapter,TCTOKSH.COM,IE0
^Thomas-Conrad TC4046 adapter,TCTOKSH.COM,00M,0051
?Select the options that match your adapter's settings.
!RIE0(INT)Hardware Interrupt
If you have a TC4035 or TC4045 half-size adapter, INT 4 is not available.
@2
3
4
5
6
7
10
11
12
!RIE0(PORT)Base I/O Address
?1A20 is primary, 2A20 is secondary, and the rest are extended addresses.
@1A20
2A20
3A20
3A40
3A60
3A80
3AA0
4AE0
!O00M(SLOT) Slot
?If "None" is selected, the driver will check the configuration for a slot number.
1
2
3
4
5
6
7
8
!OIE0(DMA)DMA Channel
?DMA 1 is not available on the TC4035 or TC4045 full-length adapter.
1
@5
6
7
!OIE0(SPEED)Line Speed (in Mbps)
?Select "None" to follow the TC4045 adapter's jumper setting.  To override the jumper setting, make another selection.
4
16
$OIEM(MAX FRAME SIZE)Maximum Frame Size
?Select Maximum Frame Size. Default: 4216. Larger frame sizes may improve performance. MAX FRAME SIZE above 4216 is allowed only if Speed is set at 16 Mbps.
618
17690
!OIE0()Non-DMA (non-bus-mastering) Mode
?Select NDMA to disable bus mastering. This setting should be used only in computers that do not support bus mastering or when other devices are using all available DMA channels.  NDMA overrides the DMA setting. 
NDMA
!OIEM()Disable Early Token Release
?Select DETR to disable Early Token Release for 16Mbps networks.
DETR
!OIEM()Non_VDS
?In most cases, select "None."  Use NON_VDS only with older memory management software versions that do not support Virtual DMA Services (VDS).
NON_VDS
!OIEM()Reinsert
?In most cases, select "None."  If you want the driver to reinsert into the ring after a MAC Remove Frame is received, select "Reinsert."
REINSERT
*RIEM(FRAME) Frame Type
?The driver defaults to the TOKEN-RING frame type.  TOKEN-RING_SNAP is also available.
@TOKEN-RING MSB
TOKEN-RING_SNAP MSB
$OIEM(NODE ADDRESS) Node address
?Select "None" unless you want to set a locally administered node ID in the range shown.
40000000000
40007FFFFFF
InS_EnD
