DOT                   * Include to indicate the printer being
*                    defined is a Dot Matrix Printer.
INIT 12
                        * Define up to 15 code characters to be sent to the
*                    printer each time PPRINT is started.  For customized
*                    printer initialization.
FFEED 12              * Define the code for a form feed character.
COMPON 27 81          * Codes to set compressed printing on.
COMPOFF 27 80         * Code to be sent to printer to set
*                    compressed mode off once it has been set on.
8LPI 27 66            * Code to set printer in 8 lines per inch mode.
6LPI 27 65            * Code to set printer in 8 lines per inch mode.
EMPH 27 33            * Code for printers Emhphasized mode
EMPHOFF 27 34         * Code to set printers Emhphasized mode off
ONEDIR 27 62          * Code to set one directional printing
ONEDIROFF 27 60       * Code to reset one directional printing
12CPI 27 69           * Set printers 12 char per inch printing
12CPIOFF 27 78        * Reset printers 12 char per inch printing
TOPMARGIN 8           * Set number of lines to always allow for
*                    top margin of printer.
BOTMARGIN 6           * Set number of lines to always allow for
*                    top margin of printer.
LINELEN 80            * Specify the line length PPRINT is to
*                    assume for the printer.
LINESPAGE 66          * Specify number of print lines to print per page.
PROPORTIONAL 27 80    * Code to set proportional print mode on
PROPORTIONALOFF 27 78 * Code to set proportional print mode off

