Amiga Mail_{Volume II}

Finding the Aspect Ratio

by Carolyn Scheppner

The pixel aspect ratio describes the ratio of the width (x Aspect) to height (y Aspect) of the pixels in a Screen or ViewPort. In order to create a truly What-You-See-Is-What-You-Get graphics display on the Amiga, you need to find the pixel aspect ratio of the display mode you are using. With the proper aspect ratio, an application can correctly display and store ILBM files, can rotate objects properly, and can calculate the proper dimensions to draw true circles and squares so they appear the same on the Amiga display as they would on some other output device, like a laser printer.

Under 1.3 and the original Amiga chip set, relatively few display modes were available. Under pre- 2.0 versions of the OS, applications can use hard-coded values for the X/Y pixel aspect ratio. The aspect ratios for the display modes available to the 1.3 system are ( xaspect / yaspect ):

NTSC Lores 44/52 PAL Lores 44/44

Halve the X aspect for Hires modes. Halve the Y aspect for interlaced modes.

These aspect values are more accurate than the values in the original IFF document.

On PAL displays, the pixels of Lores screens and Hires Interlace screens are square, as they have an aspect ratio of 44/44 and 22/22, respectively. To draw a square 100 pixels wide in one of these PAL modes, you could simply draw a square that is 100 pixels x 100 pixels. On a PAL Lores Interlace display, the Y resolution is doubled, making each pixel half as tall, so you would have to draw a rectangle that was 100 pixels x 200 pixels to get the same size square.

September/October 1991

Graphics

Finding the Aspect Ratio

Page V - 12

Amiga Mail_{Volume II}

On an NTSC display, pixels are not square. Pixels on a Lores NTSC screen have an aspect ratio of 44/52 (or 11/13). This means that each pixel is slightly narrower than it is high.

To draw a true square that is 100 pixels wide in an arbitrary display mode, it is necessary to calculate the correct height for the square based on the pixel aspect ratio.

    width / yAspect = height / xAspect

(in words, width is to yAspect as height is to xAspect)

If the X/Y aspect is 44/52 (Lores NTSC), the calculation would be:

    100 / 52 = height / 44

    height = (100 * 44) / 52 = 4400 / 52    /* solve for height */

Because this example uses only integer math, the ratio must be rounded to the nearest integer. A fraction a/b (where a and b are integers) rounded to the nearest integer approximately equals:

    ( a + ( b / 2 ) )  /  b

apply this to the ratio above:

    height = ( 4400 + (52>>1) ) / 52      /* with rounding */
    height = 4426/52 = 85.115384...       /* Approximate */
    height = 85                         /* truncated */

Therefore, to be square on a 44/52 aspect screen, a 100 pixel wide square would have to be 85 pixels tall.

Under 2.0 and the ECS chip set, the Amiga display is more dynamic. It has many new display modes, each of which has its own distinct pixel aspect ratio. For this reason, it is not practical nor desirable to hard code the aspect ratios for the modes that you know about (except when running under 1.3). When running under 2.0, the pixel aspect should be determined by querying the display database (see the article ‘‘An Introduction to V36 Screens and Windows’’ from the September /October 1990 issue of Amiga Mail for more information on how to query the display database). A valid DisplayInfo structure contains the X and Y aspect in the Resolution.x and Resolution.y fields. When writing an ILBM under 2.0, use these pixel aspects from the display database for the BMHD chunk’s xAspect and yAspect values.

The following example demonstrates how to determine the X and Y aspects under both release 2.0 and 1.3.

Graphics Finding the Aspect Ratio Page V - 13

Amiga Mail_{Volume II}

;/* getaspect.c - Execute me to compile me with SAS C 5.10
LC -b1 -cfistq -v -y -j73 getaspect.c
Blink FROM LIB:c.o,getaspect.o TO getaspect LIBRARY LIB:LC.lib,LIB:Amiga.lib
quit

Gets X/Y pixel aspect of a screen’s ViewPort
*/

#include <exec/types.h>
#include <exec/memory.h>
#include <libraries/dos.h>
#include <intuition/intuition.h>
#include <intuition/intuitionbase.h>
#include <graphics/displayinfo.h>
#include <graphics/gfxbase.h>

#include <clib/exec_protos.h>
#include <clib/dos_protos.h>
#include <clib/intuition_protos.h>
#include <clib/graphics_protos.h>
#include <stdlib.h>
#include <stdio.h>
#include <string.h>

#ifdef LATTICE
int CXBRK(void) { return(0); }  /* Disable Lattice CTRL/C handling */
int chkabort(void) { return(0); }  /* really */
#endif

#define MINARGS 1

UBYTE *vers = "\0$VER: getaspect 37.1";
UBYTE *Copyright =
  "getaspect v37.1\nCopyright (c) 1990 Commodore-Amiga, Inc.  All Rights Reserved";
UBYTE *usage = "Usage: getaspect";

void bye(UBYTE *s, int e);
void cleanup(void);

struct Library *IntuitionBase;
struct Library *GfxBase;

void main(int argc, char **argv)
    {
    struct Screen *first;
    struct ViewPort *vp;
    struct DisplayInfo DI;
    ULONG  modeid;
    UBYTE  xAspect, yAspect;

    if(((argc)&&(argc<MINARGS))||(argv[argc-1][0]==’?’))
    {
    printf("%s\n%s\n",Copyright,usage);
    bye("",RETURN_OK);
    }

    /* We will check later to see if we can call V36 functions */
    IntuitionBase = OpenLibrary("intuition.library",34);
    GfxBase = OpenLibrary("graphics.library",34);
    if((!IntuitionBase)||(!GfxBase))
    bye("Can’t open intuition or graphics library",RETURN_FAIL);

    printf("Using front screen’s ViewPort (for example purposes only):\n");

    first = ((struct IntuitionBase *)IntuitionBase)->FirstScreen;
    vp = &first->ViewPort;

    xAspect = 0;    /* So we can tell when we’ve got it */

    if(GfxBase->lib_Version >= 36)
    {
        modeid = GetVPModeID(vp);

        if(GetDisplayInfoData(NULL, (UBYTE *)&DI, sizeof(struct DisplayInfo),
        DTAG_DISP, modeid))
        {
        printf("Running 2.0,  ViewPort modeid is $%08lx\n",modeid);
        xAspect = DI.Resolution.x;
        yAspect = DI.Resolution.y;
        printf("Pixel  xAspect=%ld  yAspect=%ld\n",xAspect, yAspect);
        printf("PaletteRange is %ld\n",DI.PaletteRange);

Graphics

Finding the Aspect Ratio

Page V - 14

Amiga Mail_{Volume II}

        }
    }

    if(!xAspect)  /* pre-2.0 or GetDisplayInfoData failed */
    {
    modeid = vp->Modes;
    printf("Not running 2.0, ViewPort mode is $%04lx\n",modeid);
        /* default lores pixel ratio */
        xAspect = 44;
        yAspect = ((struct GfxBase *)GfxBase)->DisplayFlags & PAL  ? 44 : 52;
        if(modeid & HIRES)      xAspect = xAspect >> 1;
        if(modeid & LACE)       yAspect = yAspect >> 1;
    printf("Pixel  xAspect=%ld  yAspect=%ld\n",xAspect, yAspect);
        }

    bye("",RETURN_OK);
    }

void bye(UBYTE *s, int e)
    {
    cleanup();
    exit(e);
    }

void cleanup()
    {
    if(GfxBase) CloseLibrary(GfxBase);
    if(IntuitionBase)   CloseLibrary(IntuitionBase);
    }

∞∞