Intel EtherExpress PRO/100 EISA LAN Adapter
¬

¬Network Devices

This EISA bus device driver is designed to run on an Intel-based computer running OPENSTEPä for Mach Release 4.0.

Supported Hardware 
	Intel EtherExpress PRO/100 EISA LAN Adapter (EILA8265)

This driver supports the Intel EtherExpress PRO/100 EISA LAN Adapter which is based on the Intel 82556 LAN co-processor. The driver is capable of automatically determining the correct data rate, 10 Mbits/s or 100 Mbits/s.

Installing the Adapter  
·  	Install the adapter in the system and configure it either by using FlashStart or the EISA Configuration Utility (ECU) provided with your system.  Refer to the Intel EtherExpress PRO/100 Adapter Installation Guide for complete information.

Configuration 
·  	Log in as root and run Configure to add the adapter to the system.  
· 	Click on the Network Devices icon at the top of Configure's "Summary of Devices" window.  In the Add Network Devices panel that opens, select the radio button labeled "Show Drivers for Detected Devices" if it is not already highlighted.  
· 	Select "Intel EtherExpress PRO/100 EISA LAN Adapter" from the list, and click Add. 
·  	Select the Data Rate.  Select  "10 Mbits/s" or "100 Mbits/s" to fix the adapter to use 10Base-T or 100Base-TX respectively, or "Auto-detect" to have the driver automatically determine the data rate.
·  	Click Done, then click Save, then quit Configure.

¬
	
See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer 1824 for general information on installing and configuring device drivers.