SMC Elite Ultra ISA Ethernet Adapter
,

,Network Devices
This device driver is designed to run on an Intel-based computer running OPENSTEPä for Mach Release 4.0.

Supported Hardware: 
	SMC Elite Ultra Combo ISA Adapter (SMC8216C)
	SMC Elite Ultra Twisted Pair ISA Adapter (SMC8216T)
	SMC Elite Ultra Thin Coax ISA Adapter (SMC8216)

This driver supports the SMC Elite Ultra ISA Ethernet Adapters based on the SMC 83C790 UltraChip LAN processor.

Installation and Configuration Steps:
1. 	Install the adapter in the system, and run the EZStart provided with your adapter to ensure that the adapter is functioning correctly.  Consult  the adapter documentation for more information.
2. 	Reboot, log in as root, and run Configure.  
3.	Click on the Network Devices icon at the top of Configure's "Summary of Devices" window.  In the Add Network Devices panel that opens, click the "Show All Installed Drivers" radio button, if is not already highlighted.
4.	Select "SMC Elite Ultra Adapter" from the list, and click Add. 
5.   Choose an I/O Base Address, IRQ, and Shared RAM Base address which do not conflict with other devices on the system. 
6. 	Click Done, then click Save, then quit Configure.

,
	
See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer 1824 for general information on installing and configuring device drivers.